|  |  |  |  |
| --- | --- | --- | --- |
| **Member** | **Min Axial Force** | **Min Shear Stress** | **Min Bending Momement** |
| 2 | -6.88 N | 23.95 N | 141.92 N-mm |
| 4 | -9.72 N | -24.84 N | -1547.70 N-mm\* |
| 5 | -20.11 N | 0 N | 0 N-mm |

\* This value is potentially incorrect.

|  |  |  |  |
| --- | --- | --- | --- |
| **Member** | **Max Axial Force** | **Max Shear Stress** | **Max Bending Momement** |
| 2 | 23.95 N | 6.88 N | 104.26 N-mm |
| 4 | 0.02 N | 5.1 N | 201.41 N-mm |
| 5 | 0.59 N | 0 N | 0 N-mm |